
***w w w . i ei w or l d .c om***



**HDC-301MS**

***PCIe Mini Video/Audio Capture Card with One Channel HDMI Input, 1920x1080@30p, and H.264 Hardware Encoder***

***H.264 Hardware Encoder***

**Video Recording/Streaming**

**HDMI IN**

STB

HD camcorder

Blue-ray player

Game player Xbox360/PS4

PCIe Mini

# *Features*



***7/8.1/10***

Windows

***32/64***Bit

H.264

MPEG-4/AVC

* 1-channel HDMI input with H.264 hardware compression
* High quality video recording up to 1080p30
* Provides DirectShow filter
* Low power consumption
* Windows/Linux OS supported

***Dimensions (Unit: mm)***

# *Specifications*

30.00

11.18

Interface

|  |  |  |
| --- | --- | --- |
| Input | Video input channel | 1 channel |
| Video input type | HDMI |
| Audio input channel | 1 channel |
| Audio input type | HDMI (stereo) |

PC Interface Video Processing

|  |  |
| --- | --- |
| Type | PCIe Mini |

|  |  |
| --- | --- |
| Hardware Encoder | H.264/AVC High Profile Level 4.1 |
| Recording Datarate | Up to 30Mbps |
| Video Input Resolution | 1920 x 1080 24p/25p/30p/50p/60p  1920 x 1080 60i/59.94i/50i 1280 x 1024 30p  1280 x 800 60p 1280 x 768 60p  1280 x 720 50p/60p 1024 x 768 60p  800 x 600 60p 720 x 576 50p  720 x 480 60p 640 x 480 60p |
| Recording Formats | 1920 x 1080 24p/25p/30p 1280 x 1024 30p  1280 x 800 60p 1280 x 768 60p  1280 x 720 50p/60p 1024 x 768 60p  800 x 600 60p 720 x 576 50p  720 x 480 60p 640 x 480 60p |

Audio Processing

|  |  |
| --- | --- |
| Audio Sampling Frequencies | 44.1k, 48k Hz |
| Audio Compression | MPEG4-AAC |
| Recording Datarate | 128kbps |

System Requirement

|  |  |
| --- | --- |
| System | Intel® Core™ 2 Duo 2.4GHz or above |
| Memory | 2GB or more |

Software Support



50.93

|  |  |
| --- | --- |
| OS Support | Microsoft Windows 7/8.1/10 (32-bit & 64-bit) Linux: Ubuntu 16.04 (64-bit) (Kernel version: 4.4.0-21-generic) |
| SDK | Windows: Provides SDK and demo program with sample  source code  Linux: Provides SDK and demo program with sample source code |

Functionality

|  |  |
| --- | --- |
| Multiple Card Support | 4 cards, 4 channels |
| Scaling | Video scaling down compression |

Others

|  |  |
| --- | --- |
| Dimensions | 51 mm x 30 mm |
| Operating Temperature | 0°C ~ 60°C (32° ~ 140°F), non-condensing |
| Power Consumption | 3W |

# *Packing List*

|  |
| --- |
| 1 x HDC-301MS |
| 1 x HDMI input cable |
| 1 x QIG |

***Ordering Information***



HDC-301MS-2018-V10

***Video Capture Solutions***

|  |  |
| --- | --- |
| Part No. | Description |
| HDC-301MS-R10 | PCIe Mini video/audio capture card with one channel HDMI input, 1920x1080@30p, and H.264 hardware encoder |